# MeshCore Stats Configuration
# Copy this file to meshcore.conf and customize for your setup:
#   cp meshcore.conf.example meshcore.conf
#
# Format: KEY=value (no 'export' keyword, no spaces around '=')
# This format is compatible with both Docker env_file and shell 'source' command.
# Comments start with # and blank lines are ignored.

# =============================================================================
# Connection Settings
# =============================================================================

MESH_TRANSPORT=serial
MESH_SERIAL_PORT=/dev/ttyUSB0
# MESH_SERIAL_BAUD=115200
# MESH_DEBUG=0

# TCP transport (for macOS Docker or remote serial servers)
# MESH_TRANSPORT=tcp
# MESH_TCP_HOST=host.docker.internal
# MESH_TCP_PORT=5000

# BLE transport (Bluetooth Low Energy)
# MESH_TRANSPORT=ble
# MESH_BLE_ADDR=AA:BB:CC:DD:EE:FF
# MESH_BLE_PIN=123456

# =============================================================================
# Remote Repeater Identity
# =============================================================================
# At least REPEATER_NAME or REPEATER_KEY_PREFIX is required to identify your repeater

REPEATER_NAME=Your Repeater Name
# REPEATER_KEY_PREFIX=a1b2c3
REPEATER_PASSWORD=your-password

# =============================================================================
# Display Names (shown in UI)
# =============================================================================

REPEATER_DISPLAY_NAME=My Repeater
COMPANION_DISPLAY_NAME=My Companion

# Public key prefixes (shown below node name in sidebar, e.g., "!a1b2c3d4")
# REPEATER_PUBKEY_PREFIX=!a1b2c3d4
# COMPANION_PUBKEY_PREFIX=!e5f6g7h8

# =============================================================================
# Location Metadata (for reports and sidebar display)
# =============================================================================

REPORT_LOCATION_NAME=City, Country
REPORT_LOCATION_SHORT=City, XX
REPORT_LAT=0.0
REPORT_LON=0.0
REPORT_ELEV=0
REPORT_ELEV_UNIT=m

# =============================================================================
# Hardware Info (shown in sidebar)
# =============================================================================

REPEATER_HARDWARE=Your Repeater Model
COMPANION_HARDWARE=Your Companion Model

# =============================================================================
# Radio Configuration Presets
# =============================================================================
# Uncomment ONE preset below that matches your MeshCore configuration,
# or set custom values. These are for display purposes only.

# MeshCore EU/UK Narrow (default)
RADIO_FREQUENCY=869.618 MHz
RADIO_BANDWIDTH=62.5 kHz
RADIO_SPREAD_FACTOR=SF8
RADIO_CODING_RATE=CR8

# MeshCore EU/UK Wide
# RADIO_FREQUENCY=869.525 MHz
# RADIO_BANDWIDTH=250 kHz
# RADIO_SPREAD_FACTOR=SF10
# RADIO_CODING_RATE=CR5

# MeshCore US Standard
# RADIO_FREQUENCY=906.875 MHz
# RADIO_BANDWIDTH=250 kHz
# RADIO_SPREAD_FACTOR=SF10
# RADIO_CODING_RATE=CR5

# MeshCore US Fast
# RADIO_FREQUENCY=906.875 MHz
# RADIO_BANDWIDTH=500 kHz
# RADIO_SPREAD_FACTOR=SF7
# RADIO_CODING_RATE=CR5

# MeshCore ANZ (Australia/New Zealand)
# RADIO_FREQUENCY=917.0 MHz
# RADIO_BANDWIDTH=250 kHz
# RADIO_SPREAD_FACTOR=SF10
# RADIO_CODING_RATE=CR5

# =============================================================================
# Intervals and Timeouts
# =============================================================================

# COMPANION_STEP=60
# REPEATER_STEP=900
# REMOTE_TIMEOUT_S=10
# REMOTE_RETRY_ATTEMPTS=2
# REMOTE_RETRY_BACKOFF_S=4

# Circuit breaker settings (prevents spamming LoRa when repeater is unreachable)
# REMOTE_CB_FAILS=6
# REMOTE_CB_COOLDOWN_S=3600

# =============================================================================
# Telemetry Collection (Environmental Sensors)
# =============================================================================
# Enable telemetry collection from repeater's environmental sensors
# (temperature, humidity, barometric pressure, etc.)
# Requires sensor board attached to repeater (e.g., BME280, BME680)
# Default: 0 (disabled)
# TELEMETRY_ENABLED=1

# Telemetry-specific timeout and retry settings
# Defaults match status settings. Separate config allows tuning if telemetry
# proves problematic (e.g., firmware doesn't support it, sensor board missing).
# You can reduce these if telemetry collection is causing issues.
# TELEMETRY_TIMEOUT_S=10
# TELEMETRY_RETRY_ATTEMPTS=2
# TELEMETRY_RETRY_BACKOFF_S=4

# =============================================================================
# Paths (Native installation only)
# =============================================================================
# Docker: Leave these commented. The container uses /data/state and /out by default.
# Native: Uncomment for local cron-based installation:
# STATE_DIR=./data/state
# OUT_DIR=./out

