Please note when flashing: on the T3S3, first press reset, press the PRG button, release the reset button, release the PRG button

Write at:   
0x0 bootloader.bin   
0x8000 partitions.bin   
0xe000 boot_app0.bin   
0x10000 Programm-file   

